**0**

**START**

This button initiates a DOT screening test.

**1**

**ABORT**

This button initiates a DOT confirmation test. It can also be used to abort an ongoing test or procedure as the instrument is not asking for a numeric value.

**3**

**STAND.**

**2**

**REFUS.**

This button initiates a calibration procedure (and should only be used by used by Factory Authorized Calibration Techs). It can also be used to print a refusal result. The “refusal” feature can only be used when the AS IV is flashing SCRN or CONF.

This button starts an accuracy check procedure (calibration check).

**7**

**6**

**5**

**4**

These buttons are numbers with no secondary function.

**9**

**NO**

**8**

**YES**

The number “8” works for any required numerical date, but this button also acts as “YES” if the instrument is asking a Yes/No question.

The number “9” works for any required numerical date, but this button also acts as “NO” if the instrument is asking a Yes/No question.

Press Enter after keying in information. This button also allows you to reset the date & time.

**ENTER**

**SET**

This button allows you to toggle the RBT IV display between Date & Time and the Select Option

**---**

**Time**